Next: 4.1.2 Other Features available Up: 4.1 MCS51 variants Previous: 4.1 MCS51 variants Contents Index

## 4.1.1 pdata access by SFR

With the upcome of devices with internal xdata and flash memory devices using port P2 as dedicated I/O port is becoming more popular. Switching the high byte for pdata access which was formerly done by port P2 is then achieved by a Special Function Register. In well-established MCS51 tradition the address of this sfr is where the chip designers decided to put it. Needless to say that they didn't agree on a common name either. So that the startup code can correctly initialize xdata variables, you should define an sfr with the name _XPAGE`` at the appropriate location if the default, port P2, is not used for this. Some examples are:

> `__sfr __at (0x85) _XPAGE; /* Ramtron VRS51 family a.k.a. MPAGE */`

> `__sfr __at (0x92) _XPAGE; /* Cypress EZ-USB family, Texas Instruments (Chipcon) a.k.a. MPAGE */`

> `__sfr __at (0x91) _XPAGE; /* Infineon (Siemens) C500 family a.k.a. XPAGE */`

> `__sfr __at (0xaf) _XPAGE; /* some Silicon Labs (Cygnal) chips a.k.a. EMI0CN */`

> `__sfr __at (0xaa) _XPAGE; /* some Silicon Labs (Cygnal) chips a.k.a. EMI0CN */`

For more exotic implementations further customizations may be needed. See section 3.12 for other possibilities.

Next: 4.1.2 Other Features available Up: 4.1 MCS51 variants Previous: 4.1 MCS51 variants Contents Index